Software RAID Flash Instruction.
================================

1) Before Flash the Firmware and BIOS, please erase all the flash part first;
Boot to the Dos and run:
a:\>Clear.BAT
(It will clear all the content in the flash)

Note: Please reboot the system before doing the Firmware and BIOS flash.

2) Flash with BAT file: (Automatic flash)
a:\>***.BAT
(It will flash Firmware, BIOS and SAS address; but please manually type in the address)