# Data Object - IpPoolIpPoolConfigInfo(vim.vApp.IpPool.IpPoolConfigInfo)

Property of
  IpPool
Extends
  DynamicData
Since
  vSphere API 4.0

## Data Object Description

Specifications of either IPv4 or IPv6 configuration to be used on this network. This is a part of network configuration.

IPv4 addresses are in dot-decimal notation, e.g.: 192.0.2.235

IPv6 addresses are in colon-hexadecimal notation, e.g.: 2001:0db8:85a3::0370:7334

Properties

Name | Type | Description
--- | --- | ---
dhcpServerAvailable* | xsd:boolean | Whether a DHCP server is available on this network.
dns* | xsd:string[] | DNS servers For example: IPv4: ["10.20.0.1", "10.20.0.2"] IPv6: ["2001:0db8:85a3::0370:7334", "2001:0db8:85a3::0370:7335"] If an empty list is passed, the existing value remains unchanged. To clear this list, pass an array containing the empty string as it's only element.
gateway* | xsd:string | Gateway. This can be an empty string - if no gateway is configured. Examples: IPv4: 192.168.5.1 IPv6: 2001:0db8:85a3::1
ipPoolEnabled* | xsd:boolean | IP addresses can only be allocated from the range if the IP pool is enabled.
netmask* | xsd:string | Netmask For example: IPv4: 255.255.255.0 IPv6: ffff:ffff:ffff::
range* | xsd:string | IP range. This is specified as a set of ranges separated with commas. One range is given by a start address, a hash (#), and the length of the range. For example: 192.0.2.235 # 20 is the IPv4 range from 192.0.2.235 to 192.0.2.254 2001::7334 # 20 is the IPv6 range from 2001::7334 to 2001::7347
subnetAddress* | xsd:string | Address of the subnet. For example: IPv4: 192.168.5.0 IPv6: 2001:0db8:85a3::
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="IpPoolIpPoolConfigInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="subnetAddress" type="xsd:string" minOccurs="0"/> <element name="netmask" type="xsd:string" minOccurs="0"/> <element name="gateway" type="xsd:string" minOccurs="0"/> <element name="range" type="xsd:string" minOccurs="0"/> <element name="dns" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="dhcpServerAvailable" type="xsd:boolean" minOccurs="0"/> <element name="ipPoolEnabled" type="xsd:boolean" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>