# Data Object - UplinkPortMtuSupportEvent(vim.event.UplinkPortMtuSupportEvent)

Extends
  DvsHealthStatusChangeEvent
Since
  vSphere API 5.1

## Data Object Description

Mtu health check status of an uplink port is changed, and in the latest mtu health check, all the vlans' MTU setting on physical switch allows vSphere Distributed Switch max MTU size packets passing.

Properties

Name | Type | Description
--- | --- | ---
None
Properties inherited from DvsHealthStatusChangeEvent
healthResult, switchUuid
Properties inherited from HostEvent
None
Properties inherited from Event
chainId, changeTag, computeResource, createdTime, datacenter, ds, dvs, fullFormattedMessage, host, key, net, userName, vm
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="UplinkPortMtuSupportEvent"> <complexContent> <extension base="vsan:DvsHealthStatusChangeEvent"> <sequence> </sequence> </extension> </complexContent> </complexType>