# Data Object - HostFibreChannelOverEthernetHbaLinkInfo(vim.host.FibreChannelOverEthernetHba.LinkInfo)

Property of
  HostFibreChannelOverEthernetHba
Extends
  DynamicData
Since
  vSphere API 5.0

## Data Object Description

Represents FCoE link information. The link information represents a VNPort to VFPort Virtual Link, as described in the FC-BB-5 standard, with the addition of the VLAN ID over which a link exists.

Properties

Name | Type | Description
--- | --- | ---
fcfMac | xsd:string | FCF MAC address, also known as the VFPort MAC address in the FC-BB-5 standard. This MAC address should be of the form "xx:xx:xx:xx:xx:xx", where 'x' is a hexadecimal digit. Valid MAC addresses are unicast addresses.
vlanId | xsd:int | VLAN ID. This field represents the VLAN on which an FCoE HBA was discovered. Valid numbers fall into the range [0,4094].
vnportMac | xsd:string | VNPort MAC address, as defined by the FC-BB-5 standard. This MAC address should be of the form "xx:xx:xx:xx:xx:xx", where 'x' is a hexadecimal digit. Valid MAC addresses are unicast addresses.
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostFibreChannelOverEthernetHbaLinkInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="vnportMac" type="xsd:string"/> <element name="fcfMac" type="xsd:string"/> <element name="vlanId" type="xsd:int"/> </sequence> </extension> </complexContent> </complexType>