# Data Object - HostOpaqueSwitchPhysicalNicZone(vim.host.OpaqueSwitch.PhysicalNicZone)

Property of
  HostOpaqueSwitch
Extends
  DynamicData
Since
  vSphere API 6.0

## Data Object Description

Properties

Name | Type | Description
--- | --- | ---
key | xsd:string | The zone ID
pnicDevice* | xsd:string[] | Whenever an OpaqueSwitch is associated with a PhysicalNicZone, then by default, the zone will consist of all physical nics that are linked to the switch. However, if this property is set, then the zone will be considered to be consisting of only those physical nics that are listed here.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostOpaqueSwitchPhysicalNicZone"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="key" type="xsd:string"/> <element name="pnicDevice" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>