# Data Object - VMwareDVSMtuHealthCheckResult(vim.dvs.VmwareDistributedVirtualSwitch.MtuHealthCheckResult)

Extends
  HostMemberUplinkHealthCheckResult
See also
  NumericRange
Since
  vSphere API 5.1

## Data Object Description

This class defines MTU health check result of an uplink port in the VMware vSphered Distributed Switch.

Properties

Name | Type | Description
--- | --- | ---
mtuMismatch | xsd:boolean | True if the MTU configured in the vSphere Distributed Switch is different from the value configured in the Physical NIC, else false. If it is true, MTU health check is stopped. In this case, vlanSupportSwitchMtu and vlanNotSupportSwitchMtu will not have values.
vlanNotSupportSwitchMtu* | NumericRange[] | The vlan's MTU setting on physical switch does not allow vSphere Distributed Switch max MTU size packets passing. If the vlan is not a range, but a single Id, both start and end have the same value with the single vlan Id.
vlanSupportSwitchMtu* | NumericRange[] | The vlan's MTU setting on physical switch allows vSphere Distributed Switch max MTU size packets passing. If the vlan is not a range, but a single Id, both start and end have the same value with the single vlan Id.
Properties inherited from HostMemberUplinkHealthCheckResult
uplinkPortKey
Properties inherited from HostMemberHealthCheckResult
summary
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VMwareDVSMtuHealthCheckResult"> <complexContent> <extension base="vsan:HostMemberUplinkHealthCheckResult"> <sequence> <element name="mtuMismatch" type="xsd:boolean"/> <element name="vlanSupportSwitchMtu" type="vsan:NumericRange" minOccurs="0" maxOccurs="unbounded"/> <element name="vlanNotSupportSwitchMtu" type="vsan:NumericRange" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>