# Data Object - PhysicalNic(vim.host.PhysicalNic)

Property of
  DVSManagerPhysicalNicsList, HostNetworkInfo, HostOpaqueSwitch, HostProxySwitch, HostRdmaDevicePnicBacking, HostSriovNetworkDevicePoolInfo, HostVirtualSwitch, IscsiPortInfo
Extends
  DynamicData
See also
  FcoeConfig, HostRdmaDevice, PhysicalNicLinkInfo, PhysicalNicSpec
Since
  2.0

## Data Object Description

This data object type describes the physical network adapter as seen by the primary operating system.

Properties

Name | Type | Description
--- | --- | ---
autoNegotiateSupported* | xsd:boolean | If set the flag indicates if the physical network adapter supports autonegotiate. Since vSphere API 4.1
device | xsd:string | The device name of the physical network adapter.
dpuId* | xsd:string | The identifier of the DPU by which the physical NIC is backed. When physical NIC is not backed by DPU, dpuId will be unset. Since 8.0.0.1
driver* | xsd:string | The name of the driver. From command line: esxcli network nic get
driverVersion* | xsd:string | The version of the physical network adapter operating system driver. Since 8.0.0.1
enhancedNetworkingStackSupported* | xsd:boolean | If set the flag indicates whether a physical nic supports Enhanced Networking Stack driver Since vSphere API 6.7
ensInterruptSupported* | xsd:boolean | If set the flag indicates whether a physical nic supports Enhanced Networking Stack interrupt mode Since vSphere API 7.0
fcoeConfiguration* | FcoeConfig | The FCoE configuration of the physical network adapter. Since vSphere API 5.0
firmwareVersion* | xsd:string | The version of the firmware running in the network adapter. Since 8.0.0.1
key* | xsd:string | The linkable identifier.
linkSpeed* | PhysicalNicLinkInfo | The current link state of the physical network adapter. If this object is not set, then the link is down.
mac | xsd:string | The media access control (MAC) address of the physical network adapter. Since VI API 2.5
pci | xsd:string | Device hash of the PCI device corresponding to this physical network adapter.
rdmaDevice* | xsd:string | Associated RDMA device, if any. Since vSphere API 7.0
resourcePoolSchedulerAllowed* | xsd:boolean | Flag indicating whether the NIC allows resource pool based scheduling for network I/O control. Since vSphere API 4.1
resourcePoolSchedulerDisallowedReason* | xsd:string[] | If resourcePoolSchedulerAllowed is false, this property advertises the reason for disallowing resource scheduling on this NIC. The reasons may be one of PhysicalNicResourcePoolSchedulerDisallowedReason Since vSphere API 4.1
spec | PhysicalNicSpec | The specification of the physical network adapter.
validLinkSpecification* | PhysicalNicLinkInfo[] | The valid combinations of speed and duplexity for this physical network adapter. The speed and the duplex settings usually must be configured as a pair. This array lists all the valid combinations available for a physical network adapter. Autonegotiate is not listed as one of the combinations supported. If is implicitly supported by the physical network adapter unless autoNegotiateSupported is set to false.
vmDirectPathGen2Supported* | xsd:boolean | Deprecated. As of vSphere API 8.0. VMDirectPath Gen 2 is no longer supported and there is no replacement. Flag indicating whether the NIC supports VMDirectPath Gen 2. Note that this is only an indicator of the capabilities of this NIC, not of the whole host. If the host software is not capable of VMDirectPath Gen 2, this property will be unset, as the host cannot provide information on the NIC capability. See vmDirectPathGen2Supported Since vSphere API 4.1
vmDirectPathGen2SupportedMode* | xsd:string | Deprecated. As of vSphere API 8.0. VMDirectPath Gen 2 is no longer supported and there is no replacement. If vmDirectPathGen2Supported is true, this property advertises the VMDirectPath Gen 2 mode supported by this NIC (chosen from PhysicalNicVmDirectPathGen2SupportedMode). A mode may require that the associated vSphere Distributed Switch have a particular ProductSpec in order for network passthrough to be possible. Since vSphere API 4.1
wakeOnLanSupported | xsd:boolean | Flag indicating whether the NIC is wake-on-LAN capable Since VI API 2.5
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="PhysicalNic"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="key" type="xsd:string" minOccurs="0"/> <element name="device" type="xsd:string"/> <element name="pci" type="xsd:string"/> <element name="driver" type="xsd:string" minOccurs="0"/> <element name="driverVersion" type="xsd:string" minOccurs="0"/> <element name="firmwareVersion" type="xsd:string" minOccurs="0"/> <element name="linkSpeed" type="vsan:PhysicalNicLinkInfo" minOccurs="0"/> <element name="validLinkSpecification" type="vsan:PhysicalNicLinkInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="spec" type="vsan:PhysicalNicSpec"/> <element name="wakeOnLanSupported" type="xsd:boolean"/> <element name="mac" type="xsd:string"/> <element name="fcoeConfiguration" type="vsan:FcoeConfig" minOccurs="0"/> <element name="vmDirectPathGen2Supported" type="xsd:boolean" minOccurs="0"/> <element name="vmDirectPathGen2SupportedMode" type="xsd:string" minOccurs="0"/> <element name="resourcePoolSchedulerAllowed" type="xsd:boolean" minOccurs="0"/> <element name="resourcePoolSchedulerDisallowedReason" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="autoNegotiateSupported" type="xsd:boolean" minOccurs="0"/> <element name="enhancedNetworkingStackSupported" type="xsd:boolean" minOccurs="0"/> <element name="ensInterruptSupported" type="xsd:boolean" minOccurs="0"/> <element name="rdmaDevice" type="xsd:string" minOccurs="0"/> <element name="dpuId" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>