# Data Object - DvsIpNetworkRuleQualifier(vim.dvs.TrafficRule.IpQualifier)

Extends
  DvsNetworkRuleQualifier
See also
  DvsIpPort, IntExpression, IpAddress
Since
  vSphere API 5.5

## Data Object Description

This class defines the IP Rule Qualifier. Here IP addresses of source and destination will be used for classifying packets.

Properties

Name | Type | Description
--- | --- | ---
destinationAddress* | IpAddress | IP qualifier for destination. If this property is NULL, it will match "any IPv4 or any IPv6 address".
destinationIpPort* | DvsIpPort | Destination IP Port.
protocol* | IntExpression | Protocols like TCP, UDP, ICMP etc. The valid value for a protocol is got from IANA assigned value for the protocol. This can be got from RFC 5237 and IANA website section related to protocol numbers.
sourceAddress* | IpAddress | IP qualifier for source. If this property is NULL, it will match "any IPv4 or any IPv6 address".
sourceIpPort* | DvsIpPort | Source IP Port.
tcpFlags* | IntExpression | TCP flags. The valid values can be found at RFC 3168. TCP flags are not supported by Traffic Filtering
Properties inherited from DvsNetworkRuleQualifier
key
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="DvsIpNetworkRuleQualifier"> <complexContent> <extension base="vsan:DvsNetworkRuleQualifier"> <sequence> <element name="sourceAddress" type="vsan:IpAddress" minOccurs="0"/> <element name="destinationAddress" type="vsan:IpAddress" minOccurs="0"/> <element name="protocol" type="vsan:IntExpression" minOccurs="0"/> <element name="sourceIpPort" type="vsan:DvsIpPort" minOccurs="0"/> <element name="destinationIpPort" type="vsan:DvsIpPort" minOccurs="0"/> <element name="tcpFlags" type="vsan:IntExpression" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>