# Data Object - DistributedVirtualSwitchPortStatistics(vim.dvs.PortStatistics)

Property of
  DVPortState
Extends
  DynamicData
Since
  vSphere API 4.0

## Data Object Description

Statistic data of a DistributedVirtualPort.

Properties

Name | Type | Description
--- | --- | ---
bytesInBroadcast | xsd:long | The number of bytes received from broadcast packets.
bytesInFromPnic* | xsd:long | The number of bytes received at a pnic on the behalf of a port's connectee (inter-host rx). Since vSphere API 6.5
bytesInMulticast | xsd:long | The number of bytes received from multicast packets.
bytesInUnicast | xsd:long | The number of bytes received from unicast packets.
bytesOutBroadcast | xsd:long | The number of bytes forwarded from broadcast packets.
bytesOutMulticast | xsd:long | The number of bytes forwarded from multicast packets.
bytesOutToPnic* | xsd:long | The number of bytes transmitted at a pnic on the behalf of a port's connectee (inter-host tx). Since vSphere API 6.5
bytesOutUnicast | xsd:long | The number of bytes forwarded from unicast packets.
packetsInBroadcast | xsd:long | The number of broadcast packets received.
packetsInDropped | xsd:long | The number of received packets dropped.
packetsInException | xsd:long | The number of packets received that cause an exception.
packetsInMulticast | xsd:long | The number of multicast packets received.
packetsInUnicast | xsd:long | The number of unicast packets received.
packetsOutBroadcast | xsd:long | The number of broadcast packets forwarded.
packetsOutDropped | xsd:long | The number of packets to be forwarded dropped.
packetsOutException | xsd:long | The number of packets to be forwarded that cause an exception.
packetsOutMulticast | xsd:long | The number of multicast packets forwarded.
packetsOutUnicast | xsd:long | The number of unicast packets forwarded.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="DistributedVirtualSwitchPortStatistics"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="packetsInMulticast" type="xsd:long"/> <element name="packetsOutMulticast" type="xsd:long"/> <element name="bytesInMulticast" type="xsd:long"/> <element name="bytesOutMulticast" type="xsd:long"/> <element name="packetsInUnicast" type="xsd:long"/> <element name="packetsOutUnicast" type="xsd:long"/> <element name="bytesInUnicast" type="xsd:long"/> <element name="bytesOutUnicast" type="xsd:long"/> <element name="packetsInBroadcast" type="xsd:long"/> <element name="packetsOutBroadcast" type="xsd:long"/> <element name="bytesInBroadcast" type="xsd:long"/> <element name="bytesOutBroadcast" type="xsd:long"/> <element name="packetsInDropped" type="xsd:long"/> <element name="packetsOutDropped" type="xsd:long"/> <element name="packetsInException" type="xsd:long"/> <element name="packetsOutException" type="xsd:long"/> <element name="bytesInFromPnic" type="xsd:long" minOccurs="0"/> <element name="bytesOutToPnic" type="xsd:long" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>