# Data Object - HostNvmeOverTcpParameters(vim.host.NvmeOverTcpParameters)

Extends
  HostNvmeTransportParameters
Since
  vSphere API 7.0.3.0

## Data Object Description

This data object represents the transport specific parameters necessary to establish an NVME over TCP connection.

Properties

Name | Type | Description
--- | --- | ---
address | xsd:string | The address of the connection target. It is expected to be an IPv4 or IPv6 address.
digestVerification* | xsd:string | Digest verification parameter. When used in a discovery or connect spec, this parameter specifies the requested digest verification setting. The list of supported values is described in HostDigestVerificationSetting. If unset, a default value of disabled is assumed. For details, see: NVM Express Technical Proposal 8000 - NVMe/TCP Transport, Section 7.4.10.2, "Initialize Connection Request PDU (ICReq)" - DGST field. When part of HostNvmeDiscoveryLogEntry, this value is unset.
portNumber* | xsd:int | The port number of the TCP target port. If this field is unset, the default value of 8009 is assumed as per the IANA assignment: https://www.iana.org/assignments/service-names-port-numbers/service-names-port-numbers.xhtml
Properties inherited from HostNvmeTransportParameters
None
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostNvmeOverTcpParameters"> <complexContent> <extension base="vsan:HostNvmeTransportParameters"> <sequence> <element name="address" type="xsd:string"/> <element name="portNumber" type="xsd:int" minOccurs="0"/> <element name="digestVerification" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>