# Managed Object - VsanUpdateManager(vim.host.VsanUpdateManager)

See also
  ComputeResource, HostMaintenanceSpec, Task, VsanHclFirmwareUpdateSpec, VsanVibInstallPreflightStatus, VsanVibScanResult, VsanVibSpec
Since
  vSAN API 6.6

## Managed Object Description

Generic engine that can install VIBs onto ESX (optimized for vSAN clusters) using either rolling installs or one-shot. In addition to VIBs, it can also install firmware updates for select hardware. The Managed Entity can be accessed through MOID of vsan-update-manager, through vSAN service at ESXi host side.

Properties

Name | Type | Description
--- | --- | ---
None

Methods

Methods defined in this Managed Object
VsanVibInstall_Task, VsanVibInstallPreflightCheck, VsanVibScan

# VsanVibInstall_Task(vsanVibInstall)

Deprecated. As of vSphere API 8.0.

Takes a list of VIBs, firmwares, and installs those VIBs/FWs on the hosts referenced in the VIB/FW specs. If a scan has previously been performed, the results can be passed in. If not provided, a scan is done implicitly. Install may require ESX maintenance mode, and reboots, depending on the VIB to be installed and the state of the host. Any firmware update will always require maintenance mode and a host reboot.

Required Privileges
  None

Parameters

Name | Type | Description
--- | --- | ---
_this | ManagedObjectReference | A reference to the VsanUpdateManager used to make the method call.
cluster* P | ManagedObjectReference to a ComputeResource | Optional cluster this scan is happening in reference to. Since vSAN API 6.6
vibSpecs* P | VsanVibSpec[] | List of VIB specs to installed (context is always a single host) Since vSAN API 6.6
scanResults* P | VsanVibScanResult[] | List of VIB scan results obtained from VsanVibScan() Since vSAN API 6.6
firmwareSpecs* P | VsanHclFirmwareUpdateSpec[] | List of Firmware spec to be installed (context is always a single host and vmhba) Since vSAN API 6.6
maintenanceSpec* P | HostMaintenanceSpec | Maintenance spec to pass to EnterMaintenanceMode_Task() In case of non-rolling installs, no other vSAN action than 'noAction' is allowed. Since vSAN API 6.6
rolling* P | xsd:boolean | True (default) means a 1-host-at-a-time rolling install will be performed. Since vSAN API 6.6
noSigCheck* P | xsd:boolean | Skip signature checking, should not be used outside of fully trusted test environments. Default: False Since vSAN API 6.6

*Need not be set P Required privilege - see tooltip for details

Return Value

Type | Description
--- | ---
ManagedObjectReference to a Task |

Faults

Type | Description
--- | ---
NotFound |
NotSupported |
RuntimeFault | Thrown if any type of runtime fault is thrown that is not covered by the other faults; for example, a communication error.
VsanFault |

Events

Type
None

# VsanVibInstallPreflightCheck(vsanVibInstallPreflightCheck)

Performs pre-flight checks for a VIB install. Details of checks performed are documented in the result structure.

Required Privileges
  None

Parameters

Name | Type | Description
--- | --- | ---
_this | ManagedObjectReference | A reference to the VsanUpdateManager used to make the method call.
cluster* P | ManagedObjectReference to a ComputeResource | Cluster for which to perform preflight check Since vSAN API 6.6

*Need not be set P Required privilege: cluster

Return Value

Type | Description
--- | ---
VsanVibInstallPreflightStatus | Preflight check results

Faults

Type | Description
--- | ---
NotFound |
RuntimeFault | Thrown if any type of runtime fault is thrown that is not covered by the other faults; for example, a communication error.
VsanFault |

Events

Type
None

Show WSDL type definition
<element xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanVibInstallPreflightCheck" type="vsan:VsanVibInstallPreflightCheckRequestType"/> <element xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanVibInstallPreflightCheckResponse"> <complexType> <sequence> <element name="returnval" type="vsan:VsanVibInstallPreflightStatus"/> </sequence> </complexType> </element>

# VsanVibScan(vsanVibScan)

Takes a list of VIBs and a list of hosts, and determines which VIBs would be installed, what the requirements are (e.g. maintenance mode, reboot) and which existing VIBs (if any) they are overriding. Doesn't perform any actual install, but instead just provides information on "what if".

Required Privileges
  None

Parameters

Name | Type | Description
--- | --- | ---
_this | ManagedObjectReference | A reference to the VsanUpdateManager used to make the method call.
cluster* P | ManagedObjectReference to a ComputeResource | Optional cluster this scan is happening in reference to. Since vSAN API 6.6
vibSpecs P | VsanVibSpec[] | List of VIB specs to check (one entry per host) Since vSAN API 6.6

*Need not be set P Required privilege - see tooltip for details

Return Value

Type | Description
--- | ---
VsanVibScanResult[] | List of VIBs that would be installed. Each such result is for a single host, single VIB.

Faults

Type | Description
--- | ---
NotFound |
RuntimeFault | Thrown if any type of runtime fault is thrown that is not covered by the other faults; for example, a communication error.
VsanFault |

Events

Type
None

Show WSDL type definition
<element xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanVibScan" type="vsan:VsanVibScanRequestType"/> <element xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanVibScanResponse"> <complexType> <sequence> <element name="returnval" type="vsan:VsanVibScanResult" minOccurs="0" maxOccurs="unbounded"/> </sequence> </complexType> </element>