# Data Object - VirtualNVMEControllerOption(vim.vm.device.VirtualNVMEControllerOption)

Extends
  VirtualControllerOption
See also
  IntOption
Since
  vSphere API 6.5

## Data Object Description

VirtualNVMEControllerOption is the data object that contains the options for a virtual NVME controller.

Properties

Name | Type | Description
--- | --- | ---
numNVMEDisks | IntOption | Three properties (numNVMEDisks.min, numNVMEDisks.max, and numNVMEDisks.defaultValue) define the minimum, maximum, and default number of NVME VirtualDisk instances available at any given time in the NVME controller. The number of NVME VirtualDisk instances is also limited by the number of available namespaces in the NVME controller.
Properties inherited from VirtualControllerOption
devices, supportedDevice
Properties inherited from VirtualDeviceOption
autoAssignController, backingOption, busSlotOption, connectOption, controllerType, defaultBackingOptionIndex, deprecated, hotRemoveSupported, licensingLimit, numaSupported, plugAndPlay, type
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VirtualNVMEControllerOption"> <complexContent> <extension base="vsan:VirtualControllerOption"> <sequence> <element name="numNVMEDisks" type="vsan:IntOption"/> </sequence> </extension> </complexContent> </complexType>