# Data Object - NetIpConfigSpec(vim.net.IpConfigSpec)

Extends
  DynamicData
See also
  NetDhcpConfigSpec, NetIpConfigSpecIpAddressSpec
Since
  vSphere API 4.1

## Data Object Description

Internet Protocol Address Configuration for version 4 and version 6.

Properties

Name | Type | Description
--- | --- | ---
autoConfigurationEnabled* | xsd:boolean | Enable or disable ICMPv6 router solictitation requests from a given interface to acquire an IPv6 address and default gateway route from zero, one or more routers on the connected network.
dhcp* | NetDhcpConfigSpec | Configure client side DHCP for a given interface.
ipAddress* | NetIpConfigSpecIpAddressSpec[] | A set of manual (static) IP addresses to be configured on a given interface.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="NetIpConfigSpec"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="ipAddress" type="vsan:NetIpConfigSpecIpAddressSpec" minOccurs="0" maxOccurs="unbounded"/> <element name="dhcp" type="vsan:NetDhcpConfigSpec" minOccurs="0"/> <element name="autoConfigurationEnabled" type="xsd:boolean" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>