# Data Object - VsanNetworkConfigVdsScopeIssue(vim.vsan.VsanNetworkConfigVdsScopeIssue)

Extends
  VsanNetworkConfigBaseIssue
See also
  DistributedVirtualSwitch, HostSystem
Since
  vSAN API 6.6

## Data Object Description

Configuration issue: A cluster uses a Virtual Distributed Switch (VDS) that covers parts but not all cluster hosts. It is recommended to have all hosts in a cluster connected to the same VDS for centralized configuration management.

Properties

Name | Type | Description
--- | --- | ---
memberHosts | ManagedObjectReference[] to a HostSystem[] | Hosts which are members of the VDS.
nonMemberHosts | ManagedObjectReference[] to a HostSystem[] | Hosts which are not members of the VDS.
vds | ManagedObjectReference to a DistributedVirtualSwitch | The Virtual Distributed Switch.
Properties inherited from VsanNetworkConfigBaseIssue
None
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanNetworkConfigVdsScopeIssue"> <complexContent> <extension base="vsan:VsanNetworkConfigBaseIssue"> <sequence> <element name="vds" type="vsan:ManagedObjectReference"/> <element name="memberHosts" type="vsan:ManagedObjectReference" maxOccurs="unbounded"/> <element name="nonMemberHosts" type="vsan:ManagedObjectReference" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>