# Data Object - HostIpRouteEntry(vim.host.IpRouteEntry)

Property of
  HostIpRouteOp, HostIpRouteTableInfo
Extends
  DynamicData
Since
  vSphere API 4.0

## Data Object Description

IpRouteEntry. Routing entries are individual static routes which combined with the default route form all of the routing rules for a host.

Properties

Name | Type | Description
--- | --- | ---
deviceName* | xsd:string | If available the property indicates the device associated with the routing entry. This property can only be read from the server. It will be ignored if set by the client. Since vSphere API 4.1
gateway | xsd:string | Gateway for the routing entry
network | xsd:string | Network of the routing entry Of the format "10.20.120.0" or "2001:db8::1428:57"
prefixLength | xsd:int | Prefix length of the network (this is the 22 in 10.20.120.0/22)
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostIpRouteEntry"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="network" type="xsd:string"/> <element name="prefixLength" type="xsd:int"/> <element name="gateway" type="xsd:string"/> <element name="deviceName" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>