# Data Object - VMwareDvsLacpCapability(vim.dvs.VmwareDistributedVirtualSwitch.LacpFeatureCapability)

Property of
  VMwareDVSFeatureCapability
Extends
  DynamicData
Since
  vSphere API 5.1

## Data Object Description

The feature capabilities of Link Aggregation Control Protocol supported by the vSphere Distributed Switch.

Properties

Name | Type | Description
--- | --- | ---
lacpFastModeSupported* | xsd:boolean | Flag to indicate whether LACP Fast Mode is supported on the vSphere Distributed Switch. LACP Fast Mode is supported in vSphere Distributed Switch Version 7.0 or later. Since vSphere API 7.0.2.0
lacpSupported* | xsd:boolean | Flag to indicate whether Link Aggregation Control Protocol is supported on the vSphere Distributed Switch.
multiLacpGroupSupported* | xsd:boolean | Flag to indicate whether the vSphere Distributed Switch supports more than one Link Aggregation Control Protocol group to be configured. It is suppported in vSphere Distributed Switch Version 5.5 or later. Since vSphere API 5.5
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VMwareDvsLacpCapability"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="lacpSupported" type="xsd:boolean" minOccurs="0"/> <element name="multiLacpGroupSupported" type="xsd:boolean" minOccurs="0"/> <element name="lacpFastModeSupported" type="xsd:boolean" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>