# Data Object - HostIpRouteConfig(vim.host.IpRouteConfig)

Property of
  HostNetStackInstance, HostNetworkConfig, HostNetworkInfo, HostNetworkSystem, HostVirtualNicIpRouteSpec
Parameter to
  UpdateConsoleIpRouteConfig, UpdateIpRouteConfig
Extended by
  HostIpRouteConfigSpec
Extends
  DynamicData
Since
  2.0

## Data Object Description

IP Route Configuration. All IPv4 addresses, subnet addresses, and netmasks are specified as strings using dotted decimal notation. For example, "192.0.2.1". IPv6 addresses are 128-bit addresses represented as eight fields of up to four hexadecimal digits. A colon separates each field (:). For example, 2001:DB8:101::230:6eff:fe04:d9ff. The address can also consist of symbol '::' to represent multiple 16-bit groups of contiguous 0's only once in an address as described in RFC 2373.

Properties

Name | Type | Description
--- | --- | ---
defaultGateway* | xsd:string | The default gateway address.
gatewayDevice* | xsd:string | The gateway device. This applies to service console gateway only, it is ignored otherwise.
ipV6DefaultGateway* | xsd:string | The default ipv6 gateway address Since vSphere API 4.0
ipV6GatewayDevice* | xsd:string | The ipv6 gateway device. This applies to service console gateway only, it Since vSphere API 4.0
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostIpRouteConfig"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="defaultGateway" type="xsd:string" minOccurs="0"/> <element name="gatewayDevice" type="xsd:string" minOccurs="0"/> <element name="ipV6DefaultGateway" type="xsd:string" minOccurs="0"/> <element name="ipV6GatewayDevice" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>