# Data Object - HostHardwareStatusInfo(vim.host.HardwareStatusInfo)

Property of
  HealthSystemRuntime
Extends
  DynamicData
See also
  DpuStatusInfo, HostHardwareElementInfo, HostStorageElementInfo
Since
  VI API 2.5

## Data Object Description

Data object representing the status of the hardware components of the host.

Properties

Name | Type | Description
--- | --- | ---
cpuStatusInfo* | HostHardwareElementInfo[] | Status of the CPU packages
dpuStatusInfo* | DpuStatusInfo[] | Status of one or more DPU elements Since 8.0.0.1
memoryStatusInfo* | HostHardwareElementInfo[] | Status of the physical memory
storageStatusInfo* | HostStorageElementInfo[] | Status of the physical storage system
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostHardwareStatusInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="memoryStatusInfo" type="vsan:HostHardwareElementInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="cpuStatusInfo" type="vsan:HostHardwareElementInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="storageStatusInfo" type="vsan:HostStorageElementInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="dpuStatusInfo" type="vsan:DpuStatusInfo" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>