# Data Object - DpuStatusInfo(vim.host.HardwareStatusInfo.DpuStatusInfo)

Property of
  HostHardwareStatusInfo
Extends
  HostHardwareElementInfo
See also
  DpuStatusInfoOperationalInfo, HostFru
Since
  8.0.0.1

## Data Object Description

Data object describing the operational status of various DPU elements.

Properties

Name | Type | Description
--- | --- | ---
dpuId | xsd:string | Uniquely identify this DPU. Should be the VMware identifier which can be composed from pci and other identifying elements.
fru* | HostFru | The FRU this sensor monitors, if any.
sensors* | DpuStatusInfoOperationalInfo[] |
Properties inherited from HostHardwareElementInfo
name, status
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="DpuStatusInfo"> <complexContent> <extension base="vsan:HostHardwareElementInfo"> <sequence> <element name="dpuId" type="xsd:string"/> <element name="fru" type="vsan:HostFru" minOccurs="0"/> <element name="sensors" type="vsan:DpuStatusInfoOperationalInfo" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>