# Data Object - VsanInTransitEncryptionInfo(vim.vsan.host.DataInTransitEncryptionInfo)

Property of
  VsanDitEncryptionHealthSummary, VsanHostConfigInfoEx
Extends
  DynamicData
Since
  vSAN API vSAN 7.0U1

## Data Object Description

The configuration for data-in-transit encryption.

Properties

Name | Type | Description
--- | --- | ---
enabled* | xsd:boolean | Whether data-in-transit encryption is enabled in the cluster.
rekeyInterval* | xsd:int | Periodical rekeying interval in minutes. Default interval is 1440, i.e. 24 hours. Minimal interval is 30 minutes and maximum is 10080, i.e. 7 days.
transitionState* | xsd:string | Transition state is used to mark intermediate stages during encryption configuration change for a vSAN cluster. Default to 'settled'. See VsanEncryptionTransitionState
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanInTransitEncryptionInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="enabled" type="xsd:boolean" minOccurs="0"/> <element name="rekeyInterval" type="xsd:int" minOccurs="0"/> <element name="transitionState" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>