# Data Object - HostSriovInfo(vim.host.SriovInfo)

Extends
  HostPciPassthruInfo
Since
  vSphere API 5.5

## Data Object Description

This data object provides information about the state of SR-IOV device.

Properties

Name | Type | Description
--- | --- | ---
maxVirtualFunctionSupported | xsd:int | Maximum number of SRIOV virtual functions supported on this device
numVirtualFunction | xsd:int | Number of SRIOV virtual functions present on this device
numVirtualFunctionRequested | xsd:int | Number of SRIOV virtual functions requested for this device
sriovActive | xsd:boolean | Whether SRIOV is active for this device (meaning enabled + rebooted)
sriovCapable | xsd:boolean | Whether SRIOV is possible for this device
sriovEnabled | xsd:boolean | Whether SRIOV has been enabled by the user
Properties inherited from HostPciPassthruInfo
dependentDevice, hardwareLabel, id, passthruActive, passthruCapable, passthruEnabled
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostSriovInfo"> <complexContent> <extension base="vsan:HostPciPassthruInfo"> <sequence> <element name="sriovEnabled" type="xsd:boolean"/> <element name="sriovCapable" type="xsd:boolean"/> <element name="sriovActive" type="xsd:boolean"/> <element name="numVirtualFunctionRequested" type="xsd:int"/> <element name="numVirtualFunction" type="xsd:int"/> <element name="maxVirtualFunctionSupported" type="xsd:int"/> </sequence> </extension> </complexContent> </complexType>