# Data Object - LAGInfo(vim.host.LAGInfo)

Property of
  LACPInfo
Extends
  DynamicData
See also
  LAGUplinkInfo
Since
  vSAN API vSAN 7.0U3

## Data Object Description

This class describes the LAG information.

Properties

Name | Type | Description
--- | --- | ---
groupState | xsd:int | The group state of LAG.
lagName | xsd:string | The LAG name.
uplinks* | LAGUplinkInfo[] | The information of uplinks configured in the LAG.
vnics* | xsd:string[] | The name list of vSAN vmknics configured in the LAG.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="LAGInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="lagName" type="xsd:string"/> <element name="groupState" type="xsd:int"/> <element name="vnics" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="uplinks" type="vsan:LAGUplinkInfo" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>