# Data Object - VsanHclControllerInfo(vim.host.VsanHclControllerInfo)

Property of
  VsanHostHclInfo
Extends
  DynamicData
See also
  KeyValue, LocalizedMethodFault, VsanHclDiskInfo, VsanHclDriverInfo, VsanHostCimProviderInfo, VsanVcgDeviceInfo
Since
  vSphere API 5.5

## Data Object Description

Captures all vSAN HCL related information about particular SCSI/RAID controller.

Properties

Name | Type | Description
--- | --- | ---
cacheConfig* | xsd:string | This field is not used.
cacheConfigOnHcl* | xsd:string[] | Ignore this value.
cacheConfigSupported* | xsd:boolean | Ignore this value.
cimProviderInfo* | VsanHostCimProviderInfo | This field is not used.
controllerType* | xsd:string | Refer to VsanControllerType See VsanControllerType Since vSAN API vSAN 7.0U3
deviceDisplayName* | xsd:string | The human friendly product model description by which the controller announces itself, e.g., "Intel Corporation PIIX4 ...".
deviceId* | xsd:long | The deviceId of the PCI device, e.g. 48.
deviceName | xsd:string | The device name used by ESX to refer to the device right now, e.g. vmhba1.
deviceOnHcl* | xsd:boolean | If the device shows up on the HCL at all.
diskCapacity* | xsd:long | The capacity of a disk under the controller. The Unit is byte. Only applicable for devices like NVMe. Since vSAN API vSAN 7.0U3
diskMode* | xsd:string | The disk mode (all flash or hybrid) for the disks on the controller. Since vSAN API 6.6
diskModeOnHcl* | xsd:string[] | If the device shows up on the HCL, and is supported for the release of ESXi, this field will show the supported disk mode on HCL. Since vSAN API 6.6
diskModeSupported* | xsd:boolean | If the device shows up on the HCL, and is supported for the release of ESXi, this field checks if the disk mode of the controller is supported. Since vSAN API 6.6
disks* | VsanHclDiskInfo[] | Additional information about disks behind this controller, if available. Since vSAN API 6.6
driverName* | xsd:string | The name of the driver, e.g. mpt2sas.
driversOnHcl* | VsanHclDriverInfo[] | If the device shows up on the HCL, and is supported for the release of ESXi, this field will list the supported driver versions, as well as additional information for each driver, like associated firmware. Since vSAN API 6.6
driverVersion* | xsd:string | The version of the driver as reported by the driver kernel module, e.g. '4.23.01.00-9vmw'.
driverVersionsOnHcl* | xsd:string[] | If the device shows up on the HCL, and is supported for the release of ESXi, this field will list the supported driver versions.
driverVersionSupported* | xsd:boolean | If the device shows up on the HCL, and is supported for the release of ESXi, and the driver version is detected to be supported
extraInfo* | KeyValue[] | Any additional information not explicitly modeled in API. Can be used for vendor specific information about features of a controller.
fwAuxVersion* | xsd:string | Auxiliary firmware version. Some controllers use an additional firmware version, e.g. a "bundle version" or "build version". If present, its populated here. Since vSAN API 6.6
fwVersion* | xsd:string | Ignore this value.
fwVersionOnHcl* | xsd:string[] | Ignore this value.
fwVersionSupported* | xsd:boolean | Ignore this value.
issues* | LocalizedMethodFault[] | Any issues detected with the configuration of the the controller. Since vSAN API 6.6
productId* | xsd:string | The product ID of a controller. Only applicable for devices like NVMe. Since vSAN API vSAN 7.0U3
queueDepth* | xsd:long | The maximum supported queue depth for the controller. Since vSAN API 6.6
queueDepthOnHcl* | xsd:long | If the device shows up on the HCL, and is supported for the release of ESXi, this field will show the supported queue depth for the controller. Since vSAN API 6.6
queueDepthSupported* | xsd:boolean | If the device shows up on the HCL, and is supported for the release of ESX, this field checks if the controller's queue depth is supported. Since vSAN API 6.6
raidConfig* | xsd:string | This field is not used.
raidConfigOnHcl* | xsd:string[] | Ignore this value.
raidConfigSupported* | xsd:boolean | Ignore this value.
releasesOnHcl* | xsd:string[] | If the device is on the HCL, this holds the names of the supported releases.
releaseSupported* | xsd:boolean | If the device is on the HCL and the release of ESXi in use is supported.
remediableIssues* | xsd:string[] | Keys of issues which can be remediated. Since vSAN API 6.6
subDeviceId* | xsd:long | The subDeviceId of the PCI device, e.g. 5549.
subVendorId* | xsd:long | The subVendorId of the PCI device, e.g. 6518.
toolName* | xsd:string | The name of the vendor tool. E.g., perccli. Since vSAN API vSAN 6.7U3
toolVersion* | xsd:string | The version of the vendor tool. Since vSAN API vSAN 6.7U3
usedByVsan* | xsd:boolean | Used by vSAN. If not set, "True" should be assumed. Since vSAN API 6.6
userSelectedVcgId* | xsd:int | The vSAN VCG ID selected by the user. This field will be empty if user has never made a selection, or this controller has a unique mapping to its vSAN VCG entry originally. Since vSAN API vSAN 7.0U3
vcgEntryInfo* | VsanVcgDeviceInfo[] | A list of the matching models in vSAN VCG, the length of the list will be larger than 1 if this controller's PCI ID is used by other devices like NVMe on the vSAN VCG. Otherwise, the length will be 1, which means there is a unique mapping from this controller to a vSAN VCG entry. Since vSAN API vSAN 7.0U3
vendorId* | xsd:long | The vendorId of the PCI device, e.g. 4096.
vsanCompatibility* | xsd:string[] | A list of vSAN configurations supported by this controller. See VsanConfigType Since vSAN API 8.0.0.1
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanHclControllerInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="deviceName" type="xsd:string"/> <element name="deviceDisplayName" type="xsd:string" minOccurs="0"/> <element name="driverName" type="xsd:string" minOccurs="0"/> <element name="driverVersion" type="xsd:string" minOccurs="0"/> <element name="vendorId" type="xsd:long" minOccurs="0"/> <element name="deviceId" type="xsd:long" minOccurs="0"/> <element name="subVendorId" type="xsd:long" minOccurs="0"/> <element name="subDeviceId" type="xsd:long" minOccurs="0"/> <element name="extraInfo" type="vsan:KeyValue" minOccurs="0" maxOccurs="unbounded"/> <element name="deviceOnHcl" type="xsd:boolean" minOccurs="0"/> <element name="releaseSupported" type="xsd:boolean" minOccurs="0"/> <element name="releasesOnHcl" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="driverVersionsOnHcl" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="driverVersionSupported" type="xsd:boolean" minOccurs="0"/> <element name="fwVersionSupported" type="xsd:boolean" minOccurs="0"/> <element name="fwVersionOnHcl" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="cacheConfigSupported" type="xsd:boolean" minOccurs="0"/> <element name="cacheConfigOnHcl" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="raidConfigSupported" type="xsd:boolean" minOccurs="0"/> <element name="raidConfigOnHcl" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="fwVersion" type="xsd:string" minOccurs="0"/> <element name="raidConfig" type="xsd:string" minOccurs="0"/> <element name="cacheConfig" type="xsd:string" minOccurs="0"/> <element name="cimProviderInfo" type="vsan:VsanHostCimProviderInfo" minOccurs="0"/> <element name="usedByVsan" type="xsd:boolean" minOccurs="0"/> <element name="disks" type="vsan:VsanHclDiskInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="issues" type="vsan:LocalizedMethodFault" minOccurs="0" maxOccurs="unbounded"/> <element name="remediableIssues" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="driversOnHcl" type="vsan:VsanHclDriverInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="fwAuxVersion" type="xsd:string" minOccurs="0"/> <element name="queueDepth" type="xsd:long" minOccurs="0"/> <element name="queueDepthOnHcl" type="xsd:long" minOccurs="0"/> <element name="queueDepthSupported" type="xsd:boolean" minOccurs="0"/> <element name="diskMode" type="xsd:string" minOccurs="0"/> <element name="diskModeOnHcl" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="diskModeSupported" type="xsd:boolean" minOccurs="0"/> <element name="toolName" type="xsd:string" minOccurs="0"/> <element name="toolVersion" type="xsd:string" minOccurs="0"/> <element name="productId" type="xsd:string" minOccurs="0"/> <element name="diskCapacity" type="xsd:long" minOccurs="0"/> <element name="vcgEntryInfo" type="vsan:VsanVcgDeviceInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="controllerType" type="xsd:string" minOccurs="0"/> <element name="userSelectedVcgId" type="xsd:int" minOccurs="0"/> <element name="vsanCompatibility" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>