# Data Object - NetIpConfigInfo(vim.net.IpConfigInfo)

Property of
  GuestNicInfo
Extends
  DynamicData
See also
  NetDhcpConfigInfo, NetIpConfigInfoIpAddress
Since
  vSphere API 4.1

## Data Object Description

Protocol version independent address reporting data object for network interfaces.

Properties

Name | Type | Description
--- | --- | ---
autoConfigurationEnabled* | xsd:boolean | Enable or disable ICMPv6 router solictitation requests from a given interface to acquire an IPv6 address and default gateway route from zero, one or more routers on the connected network. If not set then ICMPv6 is not available on this system, See vim.host.Network.Capabilities
dhcp* | NetDhcpConfigInfo | Client side DHCP for a given interface.
ipAddress* | NetIpConfigInfoIpAddress[] | Zero, one or more manual (static) assigned IP addresses to be configured on a given interface.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="NetIpConfigInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="ipAddress" type="vsan:NetIpConfigInfoIpAddress" minOccurs="0" maxOccurs="unbounded"/> <element name="dhcp" type="vsan:NetDhcpConfigInfo" minOccurs="0"/> <element name="autoConfigurationEnabled" type="xsd:boolean" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>