# Data Object - HostFibreChannelOverEthernetTargetTransport(vim.host.FibreChannelOverEthernetTargetTransport)

Extends
  HostFibreChannelTargetTransport
Since
  vSphere API 5.0

## Data Object Description

Fibre Channel Over Ethernet transport information about a SCSI target. FCoE transport information is that of: the regular FC World Wide Node and Port Names; the VNPort MAC address and FCF MAC address which constitute a VN_Port to VF_Port Virtual Link; and the VLAN on which an FCoE target resides. More FCoE information can be found in the working draft of the T11's Fibre Channel Backbone 5 standard (FC-BB-5). The draft can be found at http://www.t11.org.

Properties

Name | Type | Description
--- | --- | ---
fcfMac | xsd:string | FCF MAC address. This MAC address should be of the form "xx:xx:xx:xx:xx:xx", where 'x' is a hexadecimal digit. Valid MAC addresses are unicast addresses.
vlanId | xsd:int | VLAN ID. Valid VLAN IDs fall within the range [0,4094].
vnportMac | xsd:string | VNPort MAC address. This MAC address should be of the form "xx:xx:xx:xx:xx:xx", where 'x' is a hexadecimal digit. Valid MAC addresses are unicast addresses.
Properties inherited from HostFibreChannelTargetTransport
nodeWorldWideName, portWorldWideName
Properties inherited from HostTargetTransport
None
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostFibreChannelOverEthernetTargetTransport"> <complexContent> <extension base="vsan:HostFibreChannelTargetTransport"> <sequence> <element name="vnportMac" type="xsd:string"/> <element name="fcfMac" type="xsd:string"/> <element name="vlanId" type="xsd:int"/> </sequence> </extension> </complexContent> </complexType>