# Data Object - VsanNicRdmaInfo(vim.host.VsanNicRdmaInfo)

Property of
  VsanHclNicInfo
Extends
  DynamicData
Since
  vSAN API vSAN 7.0U2

## Data Object Description

This class encapsulates the Data Center Bridging (DCB) configuration information for RDMA capable physical Network Interface Controller (NIC) on the host.

Properties

Name | Type | Description
--- | --- | ---
dcbEnabled* | xsd:boolean | True indicates the Data Center Bridging (DCB) mode is enabled on this physical NIC.
dcbMode* | xsd:string | The DCB mode for the physial NIC including 'CEE', 'IEEE' and 'PRE-CEE'. IEEE mode is recommended to ensure lossless transport in layer 2 environment.
pfcConfig* | xsd:string | The Priority-based Flow Control (PFC) configuration on physical NIC. To ensure lossless layer 2 environment, it's must required to control the traffic flow, which can be achieved by configuring the priority value to 3 or 4.
pfcEnabled* | xsd:boolean | True indicates the Priority-based Flow Control (PFC) is enabled on the physical NIC.
rdmaCapable* | xsd:boolean | Whether physical NIC is RDMA capable.
rdmaProtocolCapable* | xsd:string | Type of network protocol supported by RDMA. See RdmaProtocol
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanNicRdmaInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="rdmaCapable" type="xsd:boolean" minOccurs="0"/> <element name="rdmaProtocolCapable" type="xsd:string" minOccurs="0"/> <element name="dcbEnabled" type="xsd:boolean" minOccurs="0"/> <element name="dcbMode" type="xsd:string" minOccurs="0"/> <element name="pfcEnabled" type="xsd:boolean" minOccurs="0"/> <element name="pfcConfig" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>