# Data Object - VsanClusterNetworkHealthResult(vim.cluster.VsanClusterNetworkHealthResult)

Property of
  VsanClusterHealthSummary
Returned by
  VsanQueryVerifyClusterNetworkSettings
Extends
  DynamicData
See also
  VsanClusterNetworkPartitionInfo, VsanNetworkHealthResult, VsanQueryResultHostInfo
Since
  vSphere API 5.5

## Data Object Description

This class encapsulates the vSAN cluster network health test result

Properties

Name | Type | Description
--- | --- | ---
clusterInRDMAMode* | xsd:boolean | True indicates Cluster has enabled RDMA for data traffic among host. Only when all hosts in the cluster are enabled RDMA and use RoCEv2 protocol for data traffic, the cluster will be considered as RDMA mode. Since vSAN API vSAN 7.0U2
clusterInUnicastMode* | xsd:boolean | Cluster is using unicast or not. Only all host in the cluster are in unicast mode, will the cluster be identified as using unicast. Since vSAN API 6.6
hostLatencyCheckSuccess* | xsd:boolean | True if the network latency check via ping small package size is succeed from all of hosts to all other hosts. The network latency test will fail when the ping test between any of two hosts max latency over 200 ms. Since vSAN API 6.6
hostResults* | VsanNetworkHealthResult[] | Per host network health test result in the vSAN cluster
hostsCommFailure* | xsd:string[] | The host name list on which the vSAN service cannot cannot communicate with the vSAN service in vCenter.
hostsDisconnected* | xsd:string[] | The host name list which are disconnected from vCenter.
hostsInEsxMaintenanceMode* | xsd:string[] | The host name list which are in the maintenance mode.
hostsInVsanMaintenanceMode* | xsd:string[] | The host name list which are in the vSAN maintenance mode.
hostsWithVsanDisabled* | xsd:string[] | The host name list which are disabled vSAN.
infoAboutUnexpectedHosts* | VsanQueryResultHostInfo[] | Any additional information about hosts in otherHostsInVsanCluster field will be captured here. If there is no additional info available, then the host will not be listed here.
issueFound* | xsd:boolean | Whether any vSAN cluster network health issue was found
largePingTestSuccess* | xsd:boolean | True if the network ping test with large package size (9000 bytes) is succeed from all of hosts to all other hosts. The ping test will fail when the ping test between any of two hosts has lost packet
matchingIpSubnets* | xsd:boolean | Deprecated. As of vSphere API 6.7.0 Update 1 release. True if all of hosts in the vSAN cluster are in the same network subnets
matchingMulticastConfig* | xsd:boolean | True if all of hosts in the vSAN cluster have matched multicast configuration
otherHostsInVsanCluster* | xsd:string[] | The hosts UUID list which are in the vSAN cluster but cannot find in the vCenter cluster.
partitions* | VsanClusterNetworkPartitionInfo[] | The vSAN cluster partition information.
pingTestSuccess* | xsd:boolean | True if the network ping test with small package size is succeed from all of hosts to all other hosts. The ping test will fail when the ping test between any of two hosts has lost packet
potentialMulticastIssue* | xsd:boolean | True if the vSAN cluster has potential multicast issue if any one of the checks fails including if there is vSAN partition, any ping test fails, if the vSAN multicast configuration matches among all of hosts and if there is at lease one vSAN vmknic present for all of hosts.
vsanVmknicPresent* | xsd:boolean | True if at least one vSAN vmknic is found on the hosts
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanClusterNetworkHealthResult"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="hostResults" type="vsan:VsanNetworkHealthResult" minOccurs="0" maxOccurs="unbounded"/> <element name="issueFound" type="xsd:boolean" minOccurs="0"/> <element name="vsanVmknicPresent" type="xsd:boolean" minOccurs="0"/> <element name="matchingMulticastConfig" type="xsd:boolean" minOccurs="0"/> <element name="matchingIpSubnets" type="xsd:boolean" minOccurs="0"/> <element name="pingTestSuccess" type="xsd:boolean" minOccurs="0"/> <element name="largePingTestSuccess" type="xsd:boolean" minOccurs="0"/> <element name="hostLatencyCheckSuccess" type="xsd:boolean" minOccurs="0"/> <element name="potentialMulticastIssue" type="xsd:boolean" minOccurs="0"/> <element name="otherHostsInVsanCluster" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="partitions" type="vsan:VsanClusterNetworkPartitionInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="hostsWithVsanDisabled" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="hostsDisconnected" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="hostsCommFailure" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="hostsInEsxMaintenanceMode" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="hostsInVsanMaintenanceMode" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="infoAboutUnexpectedHosts" type="vsan:VsanQueryResultHostInfo" minOccurs="0" maxOccurs="unbounded"/> <element name="clusterInUnicastMode" type="xsd:boolean" minOccurs="0"/> <element name="clusterInRDMAMode" type="xsd:boolean" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>