# Data Object - VMwareDvsLacpGroupConfig(vim.dvs.VmwareDistributedVirtualSwitch.LacpGroupConfig)

Property of
  VMwareDVSConfigInfo, VMwareDvsLacpGroupSpec
Extends
  DynamicData
See also
  VMwareDvsLagIpfixConfig, VMwareDvsLagVlanConfig
Since
  vSphere API 5.5

## Data Object Description

This class defines VMware specific multiple IEEE 802.3ad Dynamic Link Aggregation Control Protocol groups.

Properties

Name | Type | Description
--- | --- | ---
ipfix* | VMwareDvsLagIpfixConfig | Ipfix configuration of the Link Aggregation Control Protocol group.
key* | xsd:string | The generated key as the identifier for the Link Aggregation group.
loadbalanceAlgorithm* | xsd:string | Load balance policy. See LacpLoadBalanceAlgorithm for valid values.
mode* | xsd:string | The mode of Link Aggregation Control Protocol. See UplinkLacpMode for valid values.
name* | xsd:string | The display name.
timeoutMode* | xsd:string | The timeout mode of LACP group. See UplinkLacpTimeoutMode for valid values. Since vSphere API 7.0.2.0
uplinkName* | xsd:string[] | Names for the Uplink Ports in the group. This property is ignored in an update operation.
uplinkNum* | xsd:int | The number of uplink ports.
uplinkPortKey* | xsd:string[] | Keys for the Uplink Ports in the group. This property is ignored in an update operation.
vlan* | VMwareDvsLagVlanConfig | The VLAN Specification of the Uplink Ports in the Link Aggregation group.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VMwareDvsLacpGroupConfig"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="key" type="xsd:string" minOccurs="0"/> <element name="name" type="xsd:string" minOccurs="0"/> <element name="mode" type="xsd:string" minOccurs="0"/> <element name="uplinkNum" type="xsd:int" minOccurs="0"/> <element name="loadbalanceAlgorithm" type="xsd:string" minOccurs="0"/> <element name="vlan" type="vsan:VMwareDvsLagVlanConfig" minOccurs="0"/> <element name="ipfix" type="vsan:VMwareDvsLagIpfixConfig" minOccurs="0"/> <element name="uplinkName" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="uplinkPortKey" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> <element name="timeoutMode" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>