# Data Object - VirtualVmxnet3Option(vim.vm.device.VirtualVmxnet3Option)

Extended by
  VirtualVmxnet3VrdmaOption
Extends
  VirtualVmxnetOption
See also
  BoolOption
Since
  vSphere API 4.0

## Data Object Description

The VirtualVmxnet3Option data object type contains the options for the VirtualVmxnet3 data object type.

Properties

Name | Type | Description
--- | --- | ---
uptv2Enabled* | BoolOption | Flag to indicate whether UPTv2(Uniform Pass-through version 2) is settable on this device. Since 8.0.0.1
Properties inherited from VirtualVmxnetOption
None
Properties inherited from VirtualEthernetCardOption
macType, supportedOUI, uptCompatibilityEnabled, vmDirectPathGen2Supported, wakeOnLanEnabled
Properties inherited from VirtualDeviceOption
autoAssignController, backingOption, busSlotOption, connectOption, controllerType, defaultBackingOptionIndex, deprecated, hotRemoveSupported, licensingLimit, numaSupported, plugAndPlay, type
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VirtualVmxnet3Option"> <complexContent> <extension base="vsan:VirtualVmxnetOption"> <sequence> <element name="uptv2Enabled" type="vsan:BoolOption" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>