# Data Object - VsanUnicastAddressInfo(vim.cluster.VsanUnicastAddressInfo)

Property of
  VsanPerfMemberInfo, VsanServerHostUnicastInfo
Extends
  DynamicData
Since
  vSAN API 6.6

## Data Object Description

Unicast address information of a cluster member. When unicast is used for vSAN clustering, we need to tell each host about the addresses information of all hosts in the cluster. These information includes the IP address, port and the vmknic. Host uses such information to communicate with others (through others' IP address). One such object represents one address information.

Properties

Name | Type | Description
--- | --- | ---
address | xsd:string | IP address of a cluster member. It could be IPv4 or IPv6 address.
port* | xsd:int | Port of a cluster member used for unicast traffic.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanUnicastAddressInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="address" type="xsd:string"/> <element name="port" type="xsd:int" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>