# Data Object - VsanNetworkConfigVswitchWithNoRedundancyIssue(vim.vsan.VsanNetworkConfigVswitchWithNoRedundancyIssue)

Extends
  VsanNetworkConfigBaseIssue
See also
  DistributedVirtualSwitch, HostSystem
Since
  vSAN API 6.6

## Data Object Description

Configuration issue: vSAN is using a vmknic on a vSwitch which doesn't have any physical NIC redundancy. This means in case of a physical NIC failure vSAN would not be able to use the vmknic any more to communicate with the remaining cluster. Note that physical NIC redundancy is a best practice, not a functional/support requirement.

Properties

Name | Type | Description
--- | --- | ---
host | ManagedObjectReference to a HostSystem | The Host on which the vmknic exists
numPnics | xsd:long | Number of configured physical NICs.
vds* | ManagedObjectReference to a DistributedVirtualSwitch | The Virtual Distributed Switch, if in-use.
vswitchName* | xsd:string | Standard virtual switch name, in case of VMware Standard Switch (VSS).
Properties inherited from VsanNetworkConfigBaseIssue
None
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanNetworkConfigVswitchWithNoRedundancyIssue"> <complexContent> <extension base="vsan:VsanNetworkConfigBaseIssue"> <sequence> <element name="host" type="vsan:ManagedObjectReference"/> <element name="vswitchName" type="xsd:string" minOccurs="0"/> <element name="vds" type="vsan:ManagedObjectReference" minOccurs="0"/> <element name="numPnics" type="xsd:long"/> </sequence> </extension> </complexContent> </complexType>