# Data Object - HostInternetScsiHbaIPProperties(vim.host.InternetScsiHba.IPProperties)

Property of
  HostInternetScsiHba
Parameter to
  UpdateInternetScsiIPProperties
Extends
  DynamicData
See also
  HostInternetScsiHbaIPv6Properties

## Data Object Description

The IP properties for the host bus adapter

Properties

Name | Type | Description
--- | --- | ---
address* | xsd:string | The current IPv4 address.
alternateDnsServerAddress* | xsd:string | The current secondary DNS address.
arpRedirectEnabled* | xsd:boolean | True if ARP Redirect is enabled Since vSphere API 4.0
defaultGateway* | xsd:string | The current IPv4 gateway.
dhcpConfigurationEnabled | xsd:boolean | True if the host bus adapter fetches its IP using DHCP.
ipv4Enabled* | xsd:boolean | True if IPv4 is enabled. Unset value will keep existing IPv4 enabled state as is. Since vSphere API 6.0
ipv6Address* | xsd:string | Deprecated. Since vSphere API 5.5 use { The current IPv6 address. Since vSphere API 4.0
ipv6DefaultGateway* | xsd:string | Deprecated. Since vSphere API 5.5 use { The current IPv6 default gateway. Since vSphere API 4.0
ipv6Enabled* | xsd:boolean | True if IPv6 is enabled. Unset value will keep existing IPv6 enabled state as is. Since vSphere API 6.0
ipv6properties* | HostInternetScsiHbaIPv6Properties | IPv6 properties. It is set only if { Since vSphere API 6.0
ipv6SubnetMask* | xsd:string | Deprecated. Since vSphere API 5.5 use { The current IPv6 subnet mask. Since vSphere API 4.0
jumboFramesEnabled* | xsd:boolean | Since vSphere API 4.0
mac* | xsd:string | The MAC address.
mtu* | xsd:int | True if the host bus adapter supports setting its MTU, (for Jumbo Frames, etc) Setting enableJumboFrames and not a numeric mtu value implies autoselection of appropriate MTU value for Jumbo Frames. Since vSphere API 4.0
primaryDnsServerAddress* | xsd:string | The current primary DNS address.
subnetMask* | xsd:string | The current IPv4 subnet mask.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostInternetScsiHbaIPProperties"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="mac" type="xsd:string" minOccurs="0"/> <element name="address" type="xsd:string" minOccurs="0"/> <element name="dhcpConfigurationEnabled" type="xsd:boolean"/> <element name="subnetMask" type="xsd:string" minOccurs="0"/> <element name="defaultGateway" type="xsd:string" minOccurs="0"/> <element name="primaryDnsServerAddress" type="xsd:string" minOccurs="0"/> <element name="alternateDnsServerAddress" type="xsd:string" minOccurs="0"/> <element name="ipv6Address" type="xsd:string" minOccurs="0"/> <element name="ipv6SubnetMask" type="xsd:string" minOccurs="0"/> <element name="ipv6DefaultGateway" type="xsd:string" minOccurs="0"/> <element name="arpRedirectEnabled" type="xsd:boolean" minOccurs="0"/> <element name="mtu" type="xsd:int" minOccurs="0"/> <element name="jumboFramesEnabled" type="xsd:boolean" minOccurs="0"/> <element name="ipv4Enabled" type="xsd:boolean" minOccurs="0"/> <element name="ipv6Enabled" type="xsd:boolean" minOccurs="0"/> <element name="ipv6properties" type="vsan:HostInternetScsiHbaIPv6Properties" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>