# Data Object - PhysicalNicLinkInfo(vim.host.PhysicalNic.LinkSpeedDuplex)

Property of
  PhysicalNic, PhysicalNicSpec
Parameter to
  UpdatePhysicalNicLinkSpeed
Extends
  DynamicData

## Data Object Description

The PhysicalNicLinkInfo data object describes the link speed and the type of duplex communication. The link speed indicates the bit rate in megabits per second. The duplex boolean indicates if the link is capable of full-duplex or half-duplex communication.

Properties

Name | Type | Description
--- | --- | ---
duplex | xsd:boolean | Flag to indicate whether or not the link is capable of full-duplex ("true") or only half-duplex ("false").
speedMb | xsd:int | Bit rate on the link.
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="PhysicalNicLinkInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="speedMb" type="xsd:int"/> <element name="duplex" type="xsd:boolean"/> </sequence> </extension> </complexContent> </complexType>