# Data Object - VMwareDVSConfigSpec(vim.dvs.VmwareDistributedVirtualSwitch.ConfigSpec)

Extends
  DVSConfigSpec
See also
  LinkDiscoveryProtocolConfig, VMwareDVSPvlanConfigSpec, VMwareDVSVspanConfigSpec, VMwareIpfixConfig
Since
  vSphere API 4.0

## Data Object Description

This class defines the VMware specific configuration for DistributedVirtualSwitch.

Properties

Name | Type | Description
--- | --- | ---
ipfixConfig* | VMwareIpfixConfig | Configuration for ipfix monitoring of the switch traffic. This must be set before ipfix monitoring can be enabled for the switch, or for any portgroup or port of the switch. See ipfixEnabled Since vSphere API 5.0
lacpApiVersion* | xsd:string | The Link Aggregation Control Protocol group version in the switch. See LacpApiVersion for valid values. Since vSphere API 5.5
linkDiscoveryProtocolConfig* | LinkDiscoveryProtocolConfig | See LinkDiscoveryProtocolConfig.
maxMtu* | xsd:int | The maximum MTU in the switch.
multicastFilteringMode* | xsd:string | The Multicast Filtering mode in the switch. See MulticastFilteringMode for valid values. Since vSphere API 6.0
pvlanConfigSpec* | VMwareDVSPvlanConfigSpec[] | The PVLAN configuration specification. A VMwareDVSPvlanMapEntry that has the same value for primaryVlanId and secondaryVlanId is referred to as a primary PVLAN entry. Otherwise, the VMwareDVSPvlanMapEntry is referred to as a secondary PVLAN entry. The pvlanType of a primary PVLAN entry must be promiscuous. A secondary PVLAN entry can have a pvlanType of either community or isolated. Primary PVLAN entries must be explicitly added. If there is no primary PVLAN entry corresponding to the primaryVlanId of a secondary PVLAN entry, a fault is thrown. While deleting a primary PVLAN entry, any associated secondary PVLAN entries must be explicitly deleted.
vspanConfigSpec* | VMwareDVSVspanConfigSpec[] | The Distributed Port Mirroring configuration specification. The VSPAN sessions in the array cannot be of the same key. Since vSphere API 5.0
Properties inherited from DVSConfigSpec
configVersion, contact, defaultPortConfig, defaultProxySwitchMaxNumPorts, description, extensionKey, host, infrastructureTrafficResourceConfig, maxPorts, name, netResourcePoolTrafficResourceConfig, networkResourceControlVersion, numStandalonePorts, policy, switchIpAddress, uplinkPortgroup, uplinkPortPolicy, vendorSpecificConfig
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VMwareDVSConfigSpec"> <complexContent> <extension base="vsan:DVSConfigSpec"> <sequence> <element name="pvlanConfigSpec" type="vsan:VMwareDVSPvlanConfigSpec" minOccurs="0" maxOccurs="unbounded"/> <element name="vspanConfigSpec" type="vsan:VMwareDVSVspanConfigSpec" minOccurs="0" maxOccurs="unbounded"/> <element name="maxMtu" type="xsd:int" minOccurs="0"/> <element name="linkDiscoveryProtocolConfig" type="vsan:LinkDiscoveryProtocolConfig" minOccurs="0"/> <element name="ipfixConfig" type="vsan:VMwareIpfixConfig" minOccurs="0"/> <element name="lacpApiVersion" type="xsd:string" minOccurs="0"/> <element name="multicastFilteringMode" type="xsd:string" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>