# Data Object - HostMultipathInfoPath(vim.host.MultipathInfo.Path)

Property of
  HostMultipathInfoLogicalUnit
Extends
  DynamicData
See also
  HostHostBusAdapter, HostMultipathInfoLogicalUnit, HostTargetTransport

## Data Object Description

The HostMultipathInfoPath data object is a storage entity that represents a topological path from a host bus adapter to a SCSI logical unit. Each path is unique although each host bus adapter/SCSI logical unit pair can have multiple paths.

Path objects are identified by a key. The specifics of how the key is formatted are dependent on the implementation. Example implementations include using strings like "vmhba1:0:0:0".

Properties

Name | Type | Description
--- | --- | ---
adapter | xsd:string | The host bus adapter at one endpoint of this path.
isWorkingPath* | xsd:boolean | A path, managed by a given path selection policy(psp) plugin, is denoted to be a Working Path if the psp plugin is likely to select the path for performing I/O in the near future. Since vSphere API 4.0
key | xsd:string | Identifier of the path.
lun | xsd:string | The logical unit at one endpoint of this path.
name | xsd:string | Name of path. Use this name to configure LogicalUnit multipathing policy using EnableMultipathPath and DisableMultipathPath.
pathState | xsd:string | Deprecated. As of VI API 4.0: System reported path states are available in state. Paths slated for I/O can be found using isWorkingPath. State of the path. Must be one of the values of MultipathState active Path can be used for I/O and is currently a working path. standby Path can be used for I/O but is not a working path or can be used if active paths fail. disabled Path has been administratively disabled. dead Path cannot be used for I/O. unknown Path is in unknown error state.
state* | xsd:string | System-reported state of the path. Must be one of the values of MultipathState active Path can be used for I/O. standby Path can be used for I/O if active paths fail. disabled Path has been administratively disabled. dead Path cannot be used for I/O. unknown Path is in unknown error state. Since vSphere API 4.0
transport* | HostTargetTransport | Transport information for the target end of the path.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostMultipathInfoPath"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="key" type="xsd:string"/> <element name="name" type="xsd:string"/> <element name="pathState" type="xsd:string"/> <element name="state" type="xsd:string" minOccurs="0"/> <element name="isWorkingPath" type="xsd:boolean" minOccurs="0"/> <element name="adapter" type="xsd:string"/> <element name="lun" type="xsd:string"/> <element name="transport" type="vsan:HostTargetTransport" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>