# Data Object - VirtualMachineTargetInfo(vim.vm.TargetInfo)

Extended by
  OpaqueNetworkTargetInfo, VirtualMachineCdromInfo, VirtualMachineDatastoreInfo, VirtualMachineDiskDeviceInfo, VirtualMachineDynamicPassthroughInfo, VirtualMachineFloppyInfo, VirtualMachineNetworkInfo, VirtualMachineParallelInfo, VirtualMachinePciPassthroughInfo, VirtualMachinePciSharedGpuPassthroughInfo, VirtualMachinePrecisionClockInfo, VirtualMachineScsiPassthroughInfo, VirtualMachineSerialInfo, VirtualMachineSgxTargetInfo, VirtualMachineSoundInfo, VirtualMachineUsbInfo, VirtualMachineVendorDeviceGroupInfo, VirtualMachineVFlashModuleInfo, VirtualMachineVgpuDeviceInfo, VirtualMachineVgpuProfileInfo
Extends
  DynamicData
Since
  2.0

## Data Object Description

The TargetInfo specified a value that can be used in the device backings to connect the virtual machine to a physical (or logical) host device.

Properties

Name | Type | Description
--- | --- | ---
configurationTag* | xsd:string[] | List of configurations that this device is available for. This is only filled out if more than one configuration is requested.
name | xsd:string | The identification of the endpoint on the host. The format of this depends on the kind of virtual device this endpoints is used for. For example, for a VirtualEthernetCard this would be a networkname, and for a VirtualCDROM it would be a device name.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vim25="urn:vim25" name="VirtualMachineTargetInfo"> <complexContent> <extension base="vim25:DynamicData"> <sequence> <element name="name" type="xsd:string"/> <element name="configurationTag" type="xsd:string" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>