# Data Object - DpuStatusInfoOperationalInfo(vim.host.HardwareStatusInfo.DpuStatusInfo.OperationalInfo)

Property of
  DpuStatusInfo
Extends
  DynamicData
See also
  ElementDescription
Since
  8.0.0.1

## Data Object Description

Sensor information provided by DPU that provides health status.

Properties

Name | Type | Description
--- | --- | ---
healthState* | ElementDescription | The health state of the element indicated by the sensor. See HostNumericSensorHealthState
reading | xsd:string | A description of the state of the sensor such as: N watts, Y RPM, or other measurement.
sensorId | xsd:string | This string uniquely identifies a sensor in the DPU.
timeStamp* | xsd:dateTime | Reports the ISO 8601 Timestamp when this sensor was last updated by management controller if the this sensor is capable of tracking when it was last updated. Property timeStampRaw, which comes from vendor firmware is convertible to DateTime, it will be provided.
units* | xsd:string | If provided by underying API, the base units in which the sensor reading is specified, "RPM", "WATTS" and so forth.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sms="urn:sms" name="DpuStatusInfoOperationalInfo"> <complexContent> <extension base="sms:DynamicData"> <sequence> <element name="sensorId" type="xsd:string"/> <element name="healthState" type="sms:ElementDescription" minOccurs="0"/> <element name="reading" type="xsd:string"/> <element name="units" type="xsd:string" minOccurs="0"/> <element name="timeStamp" type="xsd:dateTime" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>