# Data Object - FcoeConfig(vim.host.FcoeConfig)

Property of
  PhysicalNic
Extends
  DynamicData
See also
  FcoeConfigFcoeCapabilities, FcoeConfigVlanRange
Since
  vSphere API 5.0

## Data Object Description

This data object type describes an FCoE configuration as it pertains to an underlying physical NIC. Terminology is borrowed from T11's working draft of the Fibre Channel Backbone 5 standard (FC-BB-5). The draft can be found at http://www.t11.org.

Properties

Name | Type | Description
--- | --- | ---
capabilities | FcoeConfigFcoeCapabilities | Settable capabilities for this FcoeConfig.
fcoeActive | xsd:boolean | Indicates whether this FcoeConfig is "active" (has been used in conjunction with a parent physical network adapter for FCoE discovery).
priorityClass | xsd:int | 802.1p priority class used for FCoE traffic.
sourceMac | xsd:string | Source MAC address used for FCoE traffic. This MAC address is associated with the logical construct that is a physical NIC's associated underlying FCoE Controller, as defined in the FC-BB-5 standard. This MAC address should be of the form "xx:xx:xx:xx:xx:xx", where 'x' is a hexadecimal digit. Valid MAC addresses are unicast addresses.
vlanRange | FcoeConfigVlanRange[] | VLAN ranges associated with this FcoeConfig.
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vslm="urn:vslm" name="FcoeConfig"> <complexContent> <extension base="vslm:DynamicData"> <sequence> <element name="priorityClass" type="xsd:int"/> <element name="sourceMac" type="xsd:string"/> <element name="vlanRange" type="vslm:FcoeConfigVlanRange" maxOccurs="unbounded"/> <element name="capabilities" type="vslm:FcoeConfigFcoeCapabilities"/> <element name="fcoeActive" type="xsd:boolean"/> </sequence> </extension> </complexContent> </complexType>