# Data Object - DrConfigIPv6Info

Property of
  DrConfigInterfaceInfo
See also
  DrConfigIPv6Address
Since
  DrConfig API 3.0

## Data Object Description

Class that contains IPv6 info on a particular interface.

Properties

Name | Type | Description
--- | --- | ---
addresses* | DrConfigIPv6Address[] | A list of addresses to be statically assigned. Values can be available in parallel with set dhcp and autoconf.
autoconf | xsd:boolean | Address is assigned by Stateless Address Autoconfiguration (SLAAC). This option can be set to true in parallel with dhcp and static IPv6 addresses.
defaultGateway* | xsd:string | Default gateway for static IP address assignment. This configures the global IPv6 default gateway on the appliance with the specified gateway address and interface. This gateway replaces the existing default gateway configured on the appliance. However, if the gateway address is link-local, then it is added for that interface. This does not support configuration of multiple global default gateways through different interfaces.
dhcp | xsd:boolean | Address assigned by a DHCP server. This option can be set to true in parallel with autoconf and static IPv6 addresses.
interfaceName | xsd:string | Network interface, for example, "nic0" to configure.
Properties inherited from
None

*Need not be set