# Data Object - DrConfigIPv4Info

Property of
  DrConfigInterfaceInfo
Since
  DrConfig API 3.0

## Data Object Description

Structure that defines the IPv4 configuration state of a network interface.

Properties

Name | Type | Description
--- | --- | ---
address* | xsd:string | IPv4 address, for example, "10.20.80.191". Value not needed when DHCP mode.
defaultGateway* | xsd:string | IPv4 address of the default gateway. Value not needed when DHCP mode.
interfaceName | xsd:string | Interface name, for example, "nic0", "nic1".
mode | xsd:string | Address assignment mode. Value should be one of the IPv4Mode Enum.
prefix* | xsd:int | IPv4 CIDR prefix, for example , 24. See http://www.oav.net/mirrors/cidr.html for netmask-to-prefix conversion. Value not needed when DHCP mode.
Properties inherited from
None

*Need not be set