# Data Object - VsanHclNicInfo(vim.host.VsanHclNicInfo)

Property of
  VsanHostHclInfo
Extends
  VsanHclCommonDeviceInfo
See also
  VsanNicRdmaInfo
Since
  vSAN API 6.7

## Data Object Description

Captures all vSAN HCL related information about particular physical Nic.

Properties

Name | Type | Description
--- | --- | ---
rdmaConfig* | VsanNicRdmaInfo | The RDMA configuration for the RDMA capable physical NIC. Since vSAN API vSAN 7.0U2
useByVsan* | xsd:boolean | True if this physical NIC is used by vSAN. Since vSAN API vSAN 7.0U2
vmknic* | xsd:string | The name of physical NIC Since vSAN API vSAN 7.0U2
Properties inherited from VsanHclCommonDeviceInfo
deviceId, deviceName, deviceOnHcl, displayName, driverName, driversOnHcl, driverVersion, driverVersionsOnHcl, driverVersionSupported, extraInfo, fwVersion, fwVersionOnHcl, fwVersionSupported, releasesOnHcl, releaseSupported, subDeviceId, subVendorId, vendorId
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanHclNicInfo"> <complexContent> <extension base="vsan:VsanHclCommonDeviceInfo"> <sequence> <element name="vmknic" type="xsd:string" minOccurs="0"/> <element name="useByVsan" type="xsd:boolean" minOccurs="0"/> <element name="rdmaConfig" type="vsan:VsanNicRdmaInfo" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>