# Data Object - VsanProactiveRebalanceInfo(vim.vsan.ProactiveRebalanceInfo)

Property of
  VsanExtendedConfig
Extends
  DynamicData
Since
  vSAN API vSAN 6.7U3

## Data Object Description

The proactive rebalance information. Proactive Rebalance is used to maintain disk balance among the vSAN cluster. If Proactive Rebalance is enabled, vSAN automatically rebalances(moves the data among disks) the vSAN cluster when a capacity disk fullness hits proactive rebalance threshold. It includes the enable state of proactive rebalance, and its threshold.

Properties

Name | Type | Description
--- | --- | ---
enabled* | xsd:boolean | Whether proactive rebalance is enabled. If it is set to True, rebalance data movement will begin when following conditions are met within vSAN cluster, 1. Current disk fullness - lowest disk fullness > proactive threshold 2. Current disk fullness > mean disk fulless within cluster Allowed values: True if proactive rebalance is enabled; False if proactive rebalance is disabled. Default value: False
threshold* | xsd:int | Proactive relalance threshold. It indicates the extent of the imbalance the cluster can tolerate in percentage. If the disk imbalance (current disk fullness - lowest disk fullness) is below rebalance threshold, the proactive rebalance will not be triggered. Allowed values: 20 to 75. Default value: 30.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="VsanProactiveRebalanceInfo"> <complexContent> <extension base="vsan:DynamicData"> <sequence> <element name="enabled" type="xsd:boolean" minOccurs="0"/> <element name="threshold" type="xsd:int" minOccurs="0"/> </sequence> </extension> </complexContent> </complexType>