VMware vSphere Automation SDK for .NET 6.5.0

- Main Page
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

Public Member Functions
vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec Class Reference

The `Ethernet.UpdateSpec` class describes the updates to be made to the configuration of a virtual Ethernet adapter. More...

List of all members.

## Public Member Functions
| UpdateSpec ()
| Creates a default new instance.
bool | GetUptCompatibilityEnabled ()
| Flag indicating whether Universal Pass-Through (UPT) compatibility should be enabled on this virtual Ethernet adapter.
void | SetUptCompatibilityEnabled (bool?uptCompatibilityEnabled)
| Flag indicating whether Universal Pass-Through (UPT) compatibility should be enabled on this virtual Ethernet adapter.
vmware.vcenter.vm.hardware.EthernetTypes.MacAddressType | GetMacType ()
| MAC address type.
void | SetMacType (vmware.vcenter.vm.hardware.EthernetTypes.MacAddressType macType)
| MAC address type.
string | GetMacAddress ()
| MAC address.
void | SetMacAddress (string macAddress)
| MAC address.
bool | GetWakeOnLanEnabled ()
| Flag indicating whether wake-on-LAN shoud be enabled on this virtual Ethernet adapter.
void | SetWakeOnLanEnabled (bool?wakeOnLanEnabled)
| Flag indicating whether wake-on-LAN shoud be enabled on this virtual Ethernet adapter.
vmware.vcenter.vm.hardware.EthernetTypes.BackingSpec | GetBacking ()
| Physical resource backing for the virtual Ethernet adapter.
void | SetBacking (vmware.vcenter.vm.hardware.EthernetTypes.BackingSpec backing)
| Physical resource backing for the virtual Ethernet adapter.
bool | GetStartConnected ()
| Flag indicating whether the virtual device should be connected whenever the virtual machine is powered on.
void | SetStartConnected (bool?startConnected)
| Flag indicating whether the virtual device should be connected whenever the virtual machine is powered on.
bool | GetAllowGuestControl ()
| Flag indicating whether the guest can connect and disconnect the device.
void | SetAllowGuestControl (bool?allowGuestControl)
| Flag indicating whether the guest can connect and disconnect the device.
vmware.vapi.bindings.type.StructType | _GetType ()
vmware.vapi.data.StructValue | _GetDataValue ()
void | _Validate ()
bool | _HasTypeNameOf< T > ()
T | _ConvertTo< T > ()
override bool | Equals (object obj)
override int | GetHashCode ()
override string | ToString ()

## Detailed Description

The `Ethernet.UpdateSpec` class describes the updates to be made to the configuration of a virtual Ethernet adapter.

## Constructor & Destructor Documentation

vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::UpdateSpec | ( |  | ) | `[inline]`

Creates a default new instance.

## Member Function Documentation

T vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::_ConvertTo< T > | ( |  | ) | `[inline]`

Type Constraints

  T | : | vmware.vapi.bindings.IStructure |

vmware.vapi.data.StructValue vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::_GetDataValue | ( |  | ) | `[inline]`

vmware.vapi.bindings.type.StructType vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::_GetType | ( |  | ) | `[inline]`

bool vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::_HasTypeNameOf< T > | ( |  | ) | `[inline]`

Type Constraints

  T | : | vmware.vapi.bindings.IStructure |

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::_Validate | ( |  | ) | `[inline]`

override bool vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::Equals | ( | object | obj | ) | `[inline]`

bool vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetAllowGuestControl | ( |  | ) | `[inline]`

Flag indicating whether the guest can connect and disconnect the device.

vmware.vcenter.vm.hardware.EthernetTypes.BackingSpec vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetBacking | ( |  | ) | `[inline]`

Physical resource backing for the virtual Ethernet adapter.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

override int vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetHashCode | ( |  | ) | `[inline]`

string vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetMacAddress | ( |  | ) | `[inline]`

MAC address.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

vmware.vcenter.vm.hardware.EthernetTypes.MacAddressType vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetMacType | ( |  | ) | `[inline]`

MAC address type.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

bool vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetStartConnected | ( |  | ) | `[inline]`

Flag indicating whether the virtual device should be connected whenever the virtual machine is powered on.

bool vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetUptCompatibilityEnabled | ( |  | ) | `[inline]`

Flag indicating whether Universal Pass-Through (UPT) compatibility should be enabled on this virtual Ethernet adapter.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

bool vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::GetWakeOnLanEnabled | ( |  | ) | `[inline]`

Flag indicating whether wake-on-LAN shoud be enabled on this virtual Ethernet adapter.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetAllowGuestControl | ( | bool? | allowGuestControl | ) | `[inline]`

Flag indicating whether the guest can connect and disconnect the device.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetBacking | ( | vmware.vcenter.vm.hardware.EthernetTypes.BackingSpec | backing | ) | `[inline]`

Physical resource backing for the virtual Ethernet adapter.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetMacAddress | ( | string | macAddress | ) | `[inline]`

MAC address.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetMacType | ( | vmware.vcenter.vm.hardware.EthernetTypes.MacAddressType | macType | ) | `[inline]`

MAC address type.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetStartConnected | ( | bool? | startConnected | ) | `[inline]`

Flag indicating whether the virtual device should be connected whenever the virtual machine is powered on.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetUptCompatibilityEnabled | ( | bool? | uptCompatibilityEnabled | ) | `[inline]`

Flag indicating whether Universal Pass-Through (UPT) compatibility should be enabled on this virtual Ethernet adapter.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

void vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::SetWakeOnLanEnabled | ( | bool? | wakeOnLanEnabled | ) | `[inline]`

Flag indicating whether wake-on-LAN shoud be enabled on this virtual Ethernet adapter.

This field may be modified at any time, and changes will be applied the next time the virtual machine is powered on.

override string vmware::vcenter::vm::hardware::EthernetTypes::UpdateSpec::ToString | ( |  | ) | `[inline]`

The documentation for this class was generated from the following file:

- EthernetTypes.cs