1. Types
2. vcenter
3. vm
4. hardware
5. floppy

## vcenter vm hardware floppy: update spec

The `update_spec` structure describes the updates to be made to the configuration of a virtual floppy drive.

### Representations:

- JSON
- XML

{
"allow_guest_control": true,
"backing": {
"host_device": "string",
"image_file": "string",
"type": "IMAGE_FILE"
},
"start_connected": true
}
<?xml version="1.0" ?>
<ns0:UpdateSpec xmlns:ns0="http://vmware.com/vcenter/vm/hardware/floppy" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
<allow_guest_control>true</allow_guest_control>
<backing>
<image_file>string</image_file>
<type>IMAGE_FILE</type>
<host_device>string</host_device>
</backing>
<start_connected>true</start_connected>
</ns0:UpdateSpec>

#### Attributes:

Name | Type | Description
--- | --- | ---
Optional
backing | backing_spec | Physical resource backing for the virtual floppy drive. This field may only be modified if the virtual machine is not powered on or the virtual floppy drive is not connected. Optional. If unset, the value is unchanged.
start_connected | boolean | Flag indicating whether the virtual device should be connected whenever the virtual machine is powered on. Optional. If unset, the value is unchanged.
allow_guest_control | boolean | Flag indicating whether the guest can connect and disconnect the device. Optional. If unset, the value is unchanged.