1. Operations
2. vcenter
3. vm
4. hardware
5. adapter
6. scsi

## vcenter vm hardware adapter scsi: get

Returns information about a virtual SCSI adapter.

### Request:

#### HTTP request

GET https://{server}/rest/vcenter/vm/{vm}/hardware/adapter/scsi/{adapter}

#### Path Parameters

Name | Type | Description
--- | --- | ---
Required
vm | string | Virtual machine identifier.
adapter | string | Virtual SCSI adapter identifier.

### Response:

#### HTTP Status Code: 200

#### Representations:

- JSON
- XML

{
"value": {
"label": "string",
"pci_slot_number": 1,
"scsi": {
"bus": 1,
"unit": 1
},
"sharing": "NONE",
"type": "BUSLOGIC"
}
}
<?xml version="1.0" ?>
<ns0:Get-Result xmlns:ns0="http://vmware.com/vcenter/vm/hardware/adapter/scsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
<value>
<pci_slot_number>1</pci_slot_number>
<scsi>
<unit>1</unit>
<bus>1</bus>
</scsi>
<sharing>NONE</sharing>
<label>string</label>
<type>BUSLOGIC</type>
</value>
</ns0:Get-Result>

#### Response Type:

Name | Type | Description
--- | --- | ---
bold = required
value | info | Information about the specified virtual SCSI adapter.
value.label | string | Device label.
value.type | string | Adapter type. Defines the valid emulation types for a virtual SCSI adapter. Value is one of: BUSLOGIC: BusLogic host bus adapter. LSILOGIC: LSI Logic host bus adapter. LSILOGICSAS: LSI Logic SAS 1068 host bus adapter. PVSCSI: Paravirtualized host bus adapter.
value.scsi | scsi_address_info | Address of the SCSI adapter on the SCSI bus.
value.scsi.bus | long | Bus number of the adapter to which the device is attached.
value.scsi.unit | long | Unit number of the device.
value.pci_slot_number | long | Address of the SCSI adapter on the PCI bus. If the PCI address is invalid, the server will change it when the VM is started or as the device is hot added. Optional. May be unset if the virtual machine has never been powered on since the adapter was created.
value.sharing | string | Bus sharing mode. Defines the valid bus sharing modes for a virtual SCSI adapter. Value is one of: NONE: The virtual SCSI bus is not shared. VIRTUAL: The virtual SCSI bus is shared between two or more virtual machines. In this case, no physical machine is involved. PHYSICAL: The virtual SCSI bus is shared between two or more virtual machines residing on different physical hosts.

#### Errors:

HTTP Status Code | Type | Description
--- | --- | ---
500 | error | if the system reports an error while responding to the request.
404 | not_found | if the virtual machine or virtual SCSI adapter is not found.
400 | resource_inaccessible | if the virtual machine's configuration state cannot be accessed.
503 | service_unavailable | if the system is unable to communicate with a service to complete the request.
401 | unauthenticated | if the user can not be authenticated.
403 | unauthorized | if the user doesn't have the required privileges.