1. Operations
2. appliance
3. techpreview
4. monitoring
5. snmp

## appliance techpreview monitoring snmp: test

Send a warmStart notification to all configured traps and inform destinations (see RFC 3418).

### Request:

#### HTTP request

POST https://{server}/rest/appliance/techpreview/monitoring/snmp/test
No request parameters

### Response:

#### HTTP Status Code: 200

#### Representations:

- JSON
- XML

{
"value": {
"message": "string",
"success": true
}
}
<?xml version="1.0" ?>
<ns0:Test-Result xmlns:ns0="http://vmware.com/appliance/techpreview/monitoring/snmp" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
<value>
<message>string</message>
<success>true</success>
</value>
</ns0:Test-Result>

#### Response Type:

Name | Type | Description
--- | --- | ---
bold = required
value | SNMP_test_results | SNMP test result.
value.success | boolean | Set success to true/false
value.message | string | message

#### Errors:

HTTP Status Code | Type | Description
--- | --- | ---
500 | error | Generic error