# Data Object - PhysicalNic

Property of
  DVSManagerPhysicalNicsList, HostNetworkInfo, HostOpaqueSwitch, HostProxySwitch, HostRdmaDevicePnicBacking, HostSriovNetworkDevicePoolInfo, HostVirtualSwitch, IscsiPortInfo
Extends
  DynamicData
See also
  FcoeConfig, HostRdmaDevice, PhysicalNicLinkInfo, PhysicalNicSpec
Since
  null

## Data Object Description

Properties

Name | Type | Description
--- | --- | ---
autoNegotiateSupported* | xsd:boolean | Since vSphere API 4.1
device | xsd:string |
dpuId* | xsd:string | Since null
driver* | xsd:string |
driverVersion* | xsd:string | Since null
enhancedNetworkingStackSupported* | xsd:boolean | Since vSphere API 6.7
ensInterruptSupported* | xsd:boolean | Since vSphere API 7.0
fcoeConfiguration* | FcoeConfig | Since vSphere API 5.0
firmwareVersion* | xsd:string | Since null
key* | xsd:string |
linkSpeed* | PhysicalNicLinkInfo |
mac | xsd:string | Since VI API 2.5
pci | xsd:string |
rdmaDevice* | xsd:string | Since vSphere API 7.0
resourcePoolSchedulerAllowed* | xsd:boolean | Since vSphere API 4.1
resourcePoolSchedulerDisallowedReason* | xsd:string[] | Since vSphere API 4.1
spec | PhysicalNicSpec |
validLinkSpecification* | PhysicalNicLinkInfo[] |
vmDirectPathGen2Supported* | xsd:boolean | Since vSphere API 4.1
vmDirectPathGen2SupportedMode* | xsd:string | Since vSphere API 4.1
wakeOnLanSupported | xsd:boolean | Since VI API 2.5
Properties inherited from DynamicData
None

*Need not be set