# Data Object - VMwareDVSMtuHealthCheckResult

Extends
  HostMemberUplinkHealthCheckResult
See also
  NumericRange
Since
  vSphere API 5.1

## Data Object Description

Properties

Name | Type | Description
--- | --- | ---
mtuMismatch | xsd:boolean |
vlanNotSupportSwitchMtu* | NumericRange[] |
vlanSupportSwitchMtu* | NumericRange[] |
Properties inherited from HostMemberUplinkHealthCheckResult
uplinkPortKey
Properties inherited from HostMemberHealthCheckResult
summary
Properties inherited from DynamicData
None

*Need not be set