# Data Object - VirtualMachineDeviceRuntimeInfoVirtualEthernetCardRuntimeState

Extends
  VirtualMachineDeviceRuntimeInfoDeviceRuntimeState
See also
  VirtualMachineFeatureRequirement
Since
  vSphere API 4.1

## Data Object Description

Properties

Name | Type | Description
--- | --- | ---
attachmentStatus* | xsd:string | Since vSphere API 6.7
featureRequirement* | VirtualMachineFeatureRequirement[] | Since vSphere API 6.7
reservationStatus* | xsd:string | Since vSphere API 5.5
uptv2Active* | xsd:boolean | Since null
uptv2InactiveReasonOther* | xsd:string[] | Since null
uptv2InactiveReasonVm* | xsd:string[] | Since null
vmDirectPathGen2Active* | xsd:boolean |
vmDirectPathGen2InactiveReasonExtended* | xsd:string |
vmDirectPathGen2InactiveReasonOther* | xsd:string[] |
vmDirectPathGen2InactiveReasonVm* | xsd:string[] |
Properties inherited from VirtualMachineDeviceRuntimeInfoDeviceRuntimeState
None
Properties inherited from DynamicData
None

*Need not be set