D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: C1 | Firmware Version: 3.10NA |

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- VIRTUAL SERVER
- PORT FORWARDING
- APPLICATION RULES
- QOS Engine
- NETWORK FILTER
- ACCESS CONTROL
- WEBSITE FILTER
- INBOUND FILTER
- FIREWALL SETTINGS
- Routing
- ADVANCED WIRELESS
- ADVANCED NETWORK
- IPv6

# Firewall Settings

The Firewall Settings allow you to set a single computer on your network outside of the router.

## Firewall Settings

Enable SPI: |

## NAT Endpoint Filtering

| Endpoint Independent
UDP Endpoint Filtering: | Address Restricted
| Port And Address Restricted
| Endpoint Independent
TCP Endpoint Filtering: | Address Restricted
| Port And Address Restricted

## Anti-Spoof checking

Enable anti-spoof checking: |

## DMZ Host

The DMZ (Demilitarized Zone) option lets you set a single computer on your network outside of the router. If you have a computer that cannot run Internet applications successfully from behind the router, then you can place the computer into the DMZ for unrestricted Internet access.

Note: Putting a computer in the DMZ may expose that computer to a variety of security risks. Use of this option is only recommended as a last resort.

Enable DMZ Host : |
DMZ IP Address : |  |  |

## Application Level Gateway (ALG) Configuration

PPTP : |
IPSec (VPN) : |
RTSP : |
SIP : |

Helpful Hints…

Enable the DMZ option only as a last resort. If you are having trouble using an application from a computer behind the router, first try opening ports associated with the application in the Virtual Server or Port Forwarding sections.

More…

Copyright © 2004-2008 D-Link Systems, Inc.